Firmware within this folder is the basic one.  After firmware updates, IP module access way could be changed from HTTP to HTTPS; 
P.S:  The default IP of 192.168.0.10 should be certified after firmware updates according to the steps describled in  "Certificates" folder;